//Verison=2.2
//Example,Don't Delete flowing text!
//Button NIMI // Generator NIMI 
//Button NIMI 100 // Generator NIMI and Delay 100ms, 100 not is nessary
//Button INT0 // Generator INT0 and Delay 200ms
//Button RESETAMBE3000
//Button RESET3252
//Send 1 command, Receive 2 response with one is not verify.
//Command ID: CARRIER_LOST // necessary!
//Summary  // not essential, 
//Send command: 61 00 02 00 19 00 // necessary!
//Pause=300 // not essential, unit: ms; Pause 300ms after Send command
//Timeout=100 // not essential, unit: ms; if not receive '84 A9 61 ...' in 100ms after send command, Timeout error will happen!
//*Receive Data: 61 00 02 51 19 00 // not essential, receive but not verify
//Receive Data: 61 00 02 51 19 20 // not essential, receive and verify 
//.Set x = AA B0  -- Define var x ; Added in ver2.2
// ... 61 00 02 00 19 {x}   --- use the defined var, The {x} will be replaced with AA B0 
//
.Set READY_VAR = 01

Command ID:	DMR_CC
Send	Command: 84 A9 61 00 02 05 77 0d
Receive	Data:84 A9 61 00 02 05 77 00
Command ID:	DMR_FLC
Send	Command: 84 A9 61 00 04 05 76 05 05 05
Receive	Data:84 A9 61 00 02 05 76 00
//Command ID:	DMR_CALL_OPTION for 3918 controlled RF
//Send	Command: 84 A9 61 00 06 05 79 c1 00 00 00 00 
Command ID:	DMR_CALL_OPTION
Send	Command: 84 A9 61 00 06 05 79 81 00 00 00 00 
Receive	Data:84 A9 61 00 02 05 79 00
Pause 1000
Command ID:	WORK_MODE_TX
Send	Command: 84 A9 61 00 04 00 18 03 00 00
Receive	Data:84 A9 61 00 02 00 18 00
Command ID:	PROCESS_MODE
Send	Command: 84 A9 61 00 02 00 1A 03
Receive	Data:84 A9 61 00 02 00 1A 00

Command ID: DPMR_CALLED_ID
Send command: 84 A9 61 00 05 05 7d  01 23 45 67
Receive Data: 84 A9 61 00 02 05 7d 00
Command ID:	OWNID_BCD
Send	Command: 84 A9 61 00 05 05 7e 01 23 45 67 
Receive	Data:84 A9 61 00 02 05 7e 00

Command ID:	REPORT_FIELD
Send	Command: 84 A9 61 00 02 00 1D ff
Receive	Command:84 A9 61 00 02 00 1D 00
Command ID:	DEMOD_GAIN
Send	Command: 84 A9 61 00 03 00 1C 00 00
Receive	Command:84 A9 61 00 02 00 1C 00
Command ID:	DMR_CARRIER_LOST
Send	Command: 84 A9 61 00 02 03 19 00
Receive	Data:84 A9 61 00 02 03 19 00
Command ID:	DMR_CARRIER_READY
Send	Command: 84 A9 61 00 02 03 19 {READY_VAR}
Receive	Data:84 A9 61 00 02 03 19 00
Command ID:	DMR_CALL_START
Send	Command: 84 A9 61 00 01 05 78
Receive	Data:84 A9 61 00 02 05 78 00
Receive	Data:84 A9 61 00 02 30 7F 00
Receive	Data:84 A9 61 00 02 30 1B 04
Receive	Data:84 A9 61 00 02 30 7B d1
Receive	Data:84 A9 61 00 04 30 76 05 05 05 
Receive	Data:84 A9 61 00 04 30 50 12 D6 87
Receive	Data:84 A9 61 00 04 30 51 12 D6 87
Receive	Data:84 A9 61 00 05 30 7d 01 23 45 67
Receive	Data:84 A9 61 00 05 30 7e 01 23 45 67
Receive	Data:84 A9 61 00 02 30 27 00
pause 1500
Command ID:	READ_DMR_FLC
Send	Command: 84 A9 61 00 01 25 76
Receive	Data:84 A9 61 00 04 25 76 05 05 05 
Command ID:	RFAR_DMR_FLC
Send	Command: 84 A9 61 00 01 35 76
Receive	Data:84 A9 61 00 04 35 76 05 05 05
Command ID:	READ_DMR_CC
Send	Command: 84 A9 61 00 01 25 77
Receive	Data:84 A9 61 00 02 25 77 0d
Command ID:	RFAR_DMR_CC
Send	Command: 84 A9 61 00 01 35 77
Receive	Data:84 A9 61 00 02 35 77 0d

Command ID: DPMR_CALLED_ID
Send command: 84 A9 61 00 01 25 7d 
Receive Data: 84 A9 61 00 05 25 7d 01 23 45 67 
Command ID: DPMR_CALLED_ID
Send command: 84 A9 61 00 01 35 7d 
Receive Data: 84 A9 61 00 05 35 7d 01 23 45 67 
Command ID:	OWNID_BCD
Send	Command: 84 A9 61 00 01 25 7e
Receive	Data:84 A9 61 00 05 25 7e 01 23 45 67 
Command ID:	OWNID_BCD
Send	Command: 84 A9 61 00 01 35 7e
Receive	Data:84 A9 61 00 05 35 7e 01 23 45 67 
Command ID:	DMR_CALL_STOP
Send	Command: 84 A9 61 00 01 03 21 00
Receive	Data:84 A9 61 00 02 03 21 00
Receive	Data:84 A9 61 00 02 30 1B 04
Receive	Data:84 A9 61 00 02 30 7B d2
Receive	Data:84 A9 61 00 01 30 4B
Receive	Data:84 A9 61 00 02 20 17 0A
//Receive	Data:84 A9 61 00 02 30 1B 08
Pause 360
Command ID: WORK_MODE_IDLE
Send	Command: 84 A9 61 00 04 00 18 00 00 00
Receive	Data:84 A9 61 00 02 00 18 00
Command ID:	CARRIER_LOST
Send	Command: 84 A9 61 00 02 03 19 00
Receive	Data:84 A9 61 00 02 03 19 00

Command ID:	WORK_MODE_TX
Send	Command: 84 A9 61 00 04 00 18 03 00 00
Receive	Data:84 A9 61 00 02 00 18 00
Command ID: DPMR_CALLED_ID
Send command: 84 A9 61 00 05 05 7d  01 aa aa aa
Receive Data: 84 A9 61 00 02 05 7d 00
Command ID:	OWNID_BCD
Send	Command: 84 A9 61 00 05 05 7e 01 23 45 67 
Receive	Data:84 A9 61 00 02 05 7e 00
Command ID:	DMR_CALL_START
Send	Command: 84 A9 61 00 01 05 78
Receive	Data:84 A9 61 00 02 05 78 00
pause 400
Command ID:	DMR_CARRIER_READY
Send	Command: 84 A9 61 00 02 03 19 {READY_VAR}
Receive	Data:84 A9 61 00 02 03 19 00
pause 100

Receive	Data:84 A9 61 00 02 30 7F 00
Receive	Data:84 A9 61 00 02 30 1B 05
Receive	Data:84 A9 61 00 02 30 7C D2
Receive	Data:84 A9 61 00 04 30 76 05 05 05
Receive	Data:84 A9 61 00 04 30 50 FF FF F1
Receive	Data:84 A9 61 00 04 30 51 12 D6 87
Receive	Data:84 A9 61 00 05 30 7D 01 AA AA AA
Receive	Data:84 A9 61 00 05 30 7e 01 23 45 67
Receive	Data:84 A9 61 00 02 30 27 02
pause 1500
Command ID: DPMR_CALLED_ID
Send command: 84 A9 61 00 01 25 7d 
Receive Data: 84 A9 61 00 05 25 7d 01 aa aa aa
Command ID: DPMR_CALLED_ID
Send command: 84 A9 61 00 01 35 7d 
Receive Data: 84 A9 61 00 05 35 7D 01 AA AA AA
Command ID:	OWNID_BCD
Send	Command: 84 A9 61 00 01 25 7e
Receive	Data:84 A9 61 00 05 25 7E 01 23 45 67
Command ID:	OWNID_BCD
Send	Command: 84 A9 61 00 01 35 7e
Receive	Data:84 A9 61 00 05 35 7e 01 23 45 67 
Command ID:	DMR_CALL_STOP
Send	Command: 84 A9 61 00 01 03 21 00
Receive	Data:84 A9 61 00 02 03 21 00
Receive	Data:84 A9 61 00 02 30 1B 04
Receive	Data:84 A9 61 00 02 30 7B d2
Receive	Data:84 A9 61 00 01 30 4B
Receive	Data:84 A9 61 00 02 20 17 0A
Pause 360
//Receive	Data:84 A9 61 00 02 30 1B 08
//Command ID:	CARRIER_LOST
//Send	Command: 84 A9 61 00 02 03 19 01
//Receive	Data:84 A9 61 00 02 03 19 00


Command ID:	WORK_MODE_IDLE
Send	Command: 84 A9 61 00 04 00 18 00 00 00
Receive	Data:84 A9 61 00 02 00 18 00


Command ID:	CARRIER_LOST
Send	Command: 84 A9 61 00 02 03 19 00
Receive	Data:84 A9 61 00 02 03 19 00

Command ID:	WORK_MODE_TX
Send	Command: 84 A9 61 00 04 00 18 03 00 00
Receive	Data:84 A9 61 00 02 00 18 00
Command ID: DPMR_CALLED_ID
Send command: 84 A9 61 00 05 05 7d  02 aa aa aa
Receive Data: 84 A9 61 00 02 05 7d 00
Command ID:	OWNID_BCD
Send	Command: 84 A9 61 00 05 05 7e 02 23 45 67 
Receive	Data:84 A9 61 00 02 05 7e 00
Command ID:	DMR_CARRIER_READY
Send	Command: 84 A9 61 00 02 03 19 {READY_VAR}
Receive	Data:84 A9 61 00 02 03 19 00
pause 100
Command ID:	DMR_CALL_START
Send	Command: 84 A9 61 00 01 05 78
Receive	Data:84 A9 61 00 02 05 78 00
pause 400



Receive	Data:84 A9 61 00 02 30 7F 00
Receive	Data:84 A9 61 00 02 30 1B 04
Receive	Data:84 A9 61 00 02 30 7b d1
Receive	Data:84 A9 61 00 04 30 76 05 05 05
Receive	Data:84 A9 61 00 04 30 50 FF FF F2
Receive	Data:84 A9 61 00 04 30 51 22 18 C7
Receive	Data:84 A9 61 00 05 30 7d 02 AA AA AA
Receive	Data:84 A9 61 00 05 30 7e 02 23 45 67
Receive	Data:84 A9 61 00 02 30 27 02
pause 1500
Command ID: DPMR_CALLED_ID
Send command: 84 A9 61 00 01 25 7d 
Receive Data: 84 A9 61 00 05 25 7d 02 aa aa aa
Command ID: DPMR_CALLED_ID
Send command: 84 A9 61 00 01 35 7d 
Receive Data: 84 A9 61 00 05 35 7d 02 aa aa aa

Command ID:	DMR_CALL_STOP
Send	Command: 84 A9 61 00 01 03 21 00
Receive	Data:84 A9 61 00 02 03 21 00
Receive	Data:84 A9 61 00 02 30 1B 04
Receive	Data:84 A9 61 00 02 30 7B d2
Receive	Data:84 A9 61 00 01 30 4B
Receive	Data:84 A9 61 00 02 20 17 0A
Pause 360
//Receive	Data:84 A9 61 00 02 30 1B 08
//Command ID:	CARRIER_LOST
//Send	Command: 84 A9 61 00 02 03 19 01
//Receive	Data:84 A9 61 00 02 03 19 00

Command ID:	WORK_MODE_IDLE
Send	Command: 84 A9 61 00 04 00 18 00 00 00
Receive	Data:84 A9 61 00 02 00 18 00
Command ID:	CARRIER_LOST
Send	Command: 84 A9 61 00 02 03 19 00
Receive	Data:84 A9 61 00 02 03 19 00

Command ID:	WORK_MODE_TX
Send	Command: 84 A9 61 00 04 00 18 03 00 00
Receive	Data:84 A9 61 00 02 00 18 00
Command ID: DPMR_CALLED_ID
Send command: 84 A9 61 00 05 05 7d  03 aa aa aa
Receive Data: 84 A9 61 00 02 05 7d 00
Command ID:	OWNID_BCD
Send	Command: 84 A9 61 00 05 05 7e 03 23 45 67 
Receive	Data:84 A9 61 00 02 05 7e 00
Command ID:	DMR_CALL_START
Send	Command: 84 A9 61 00 01 05 78
Receive	Data:84 A9 61 00 02 05 78 00
pause 400
Command ID:	DMR_CARRIER_READY
Send	Command: 84 A9 61 00 02 03 19 {READY_VAR}
Receive	Data:84 A9 61 00 02 03 19 00
pause 100

Receive	Data:84 A9 61 00 02 30 7F 00
Receive	Data:84 A9 61 00 02 30 1B 05
Receive	Data:84 A9 61 00 02 30 7C D2
Receive	Data:84 A9 61 00 04 30 76 05 05 05
Receive	Data:84 A9 61 00 04 30 50 FF FF F3
Receive	Data:84 A9 61 00 04 30 51 31 5B 07
Receive	Data:84 A9 61 00 05 30 7D 03 AA AA AA
Receive	Data:84 A9 61 00 05 30 7E 03 23 45 67
Receive	Data:84 A9 61 00 02 30 27 02
pause 1500
Command ID: DPMR_CALLED_ID
Send command: 84 A9 61 00 01 25 7d 
Receive Data: 84 A9 61 00 05 25 7d 03 aa aa aa
Command ID: DPMR_CALLED_ID
Send command: 84 A9 61 00 01 35 7d 
Receive Data: 84 A9 61 00 05 35 7d 03 aa aa aa
Command ID:	DMR_CALL_STOP
Send	Command: 84 A9 61 00 01 03 21 00
Receive	Data:84 A9 61 00 02 03 21 00
Receive	Data:84 A9 61 00 02 30 1B 04
Receive	Data:84 A9 61 00 02 30 7B d2
Receive	Data:84 A9 61 00 01 30 4B
Receive	Data:84 A9 61 00 02 20 17 0A
Pause 360
//Receive	Data:84 A9 61 00 02 30 1B 08
//Command ID:	CARRIER_LOST
//Send	Command: 84 A9 61 00 02 03 19 01
//Receive	Data:84 A9 61 00 02 03 19 00

Command ID:	WORK_MODE_IDLE
Send	Command: 84 A9 61 00 04 00 18 00 00 00
Receive	Data:84 A9 61 00 02 00 18 00
Command ID:	CARRIER_LOST
Send	Command: 84 A9 61 00 02 03 19 00
Receive	Data:84 A9 61 00 02 03 19 00

Command ID:	WORK_MODE_TX
Send	Command: 84 A9 61 00 04 00 18 03 00 00
Receive	Data:84 A9 61 00 02 00 18 00
Command ID: DPMR_CALLED_ID
Send command: 84 A9 61 00 05 05 7d  04 aa aa aa
Receive Data: 84 A9 61 00 02 05 7d 00
Command ID:	OWNID_BCD
Send	Command: 84 A9 61 00 05 05 7e 04 23 45 67 
Receive	Data:84 A9 61 00 02 05 7e 00
Command ID:	DMR_CARRIER_READY
Send	Command: 84 A9 61 00 02 03 19 {READY_VAR}
Receive	Data:84 A9 61 00 02 03 19 00
pause 100
Command ID:	DMR_CALL_START
Send	Command: 84 A9 61 00 01 05 78
Receive	Data:84 A9 61 00 02 05 78 00
pause 400



Receive	Data:84 A9 61 00 02 30 7F 00
Receive	Data:84 A9 61 00 02 30 1B 04
Receive	Data:84 A9 61 00 02 30 7b d1
Receive	Data:84 A9 61 00 04 30 76 05 05 05
Receive	Data:84 A9 61 00 04 30 50 FF FF F4
Receive	Data:84 A9 61 00 04 30 51 40 9D 47
Receive	Data:84 A9 61 00 05 30 7d 04 AA AA AA
Receive	Data:84 A9 61 00 05 30 7e 04 23 45 67
Receive	Data:84 A9 61 00 02 30 27 02
pause 1500
Command ID:	DMR_CALL_STOP
Send	Command: 84 A9 61 00 01 03 21 00
Receive	Data:84 A9 61 00 02 03 21 00
Receive	Data:84 A9 61 00 02 30 1B 04
Receive	Data:84 A9 61 00 02 30 7B d2
Receive	Data:84 A9 61 00 01 30 4B
Receive	Data:84 A9 61 00 02 20 17 0A
Pause 360
//Receive	Data:84 A9 61 00 02 30 1B 08
//Command ID:	CARRIER_LOST
//Send	Command: 84 A9 61 00 02 03 19 01
//Receive	Data:84 A9 61 00 02 03 19 00

Command ID:	WORK_MODE_IDLE
Send	Command: 84 A9 61 00 04 00 18 00 00 00
Receive	Data:84 A9 61 00 02 00 18 00
Command ID:	CARRIER_LOST
Send	Command: 84 A9 61 00 02 03 19 00
Receive	Data:84 A9 61 00 02 03 19 00

Command ID:	WORK_MODE_TX
Send	Command: 84 A9 61 00 04 00 18 03 00 00
Receive	Data:84 A9 61 00 02 00 18 00
Command ID: DPMR_CALLED_ID
Send command: 84 A9 61 00 05 05 7d  05 aa aa aa
Receive Data: 84 A9 61 00 02 05 7d 00
Command ID:	OWNID_BCD
Send	Command: 84 A9 61 00 05 05 7e 05 23 45 67 
Receive	Data:84 A9 61 00 02 05 7e 00
Command ID:	DMR_CALL_START
Send	Command: 84 A9 61 00 01 05 78
Receive	Data:84 A9 61 00 02 05 78 00
pause 400

Command ID:	DMR_CARRIER_READY
Send	Command: 84 A9 61 00 02 03 19 {READY_VAR}
Receive	Data:84 A9 61 00 02 03 19 00
pause 100

Receive	Data:84 A9 61 00 02 30 7F 00
Receive	Data:84 A9 61 00 02 30 1B 05
Receive	Data:84 A9 61 00 02 30 7C D2
Receive	Data:84 A9 61 00 04 30 76 05 05 05
Receive	Data:84 A9 61 00 04 30 50 FF FF F5
Receive	Data:84 A9 61 00 04 30 51 4F DF 87
Receive	Data:84 A9 61 00 05 30 7D 05 AA AA AA
Receive	Data:84 A9 61 00 05 30 7E 05 23 45 67
Receive	Data:84 A9 61 00 02 30 27 02
pause 1500
Command ID:	DMR_CALL_STOP
Send	Command: 84 A9 61 00 01 03 21 00
Receive	Data:84 A9 61 00 02 03 21 00
Receive	Data:84 A9 61 00 02 30 1B 04
Receive	Data:84 A9 61 00 02 30 7B d2
Receive	Data:84 A9 61 00 01 30 4B
Receive	Data:84 A9 61 00 02 20 17 0A
Pause 360
//Receive	Data:84 A9 61 00 02 30 1B 08
//Command ID:	CARRIER_LOST
//Send	Command: 84 A9 61 00 02 03 19 01
//Receive	Data:84 A9 61 00 02 03 19 00

Command ID:	WORK_MODE_IDLE
Send	Command: 84 A9 61 00 04 00 18 00 00 00
Receive	Data:84 A9 61 00 02 00 18 00
Command ID:	CARRIER_LOST
Send	Command: 84 A9 61 00 02 03 19 00
Receive	Data:84 A9 61 00 02 03 19 00

Command ID:	WORK_MODE_TX
Send	Command: 84 A9 61 00 04 00 18 03 00 00
Receive	Data:84 A9 61 00 02 00 18 00
Command ID: DPMR_CALLED_ID
Send command: 84 A9 61 00 05 05 7d  06 aa aa aa
Receive Data: 84 A9 61 00 02 05 7d 00
Command ID:	OWNID_BCD
Send	Command: 84 A9 61 00 05 05 7e 06 23 45 67 
Receive	Data:84 A9 61 00 02 05 7e 00
Command ID:	DMR_CALL_START
Send	Command: 84 A9 61 00 01 05 78
Receive	Data:84 A9 61 00 02 05 78 00
pause 400
Command ID:	DMR_CARRIER_READY
Send	Command: 84 A9 61 00 02 03 19 {READY_VAR}
Receive	Data:84 A9 61 00 02 03 19 00
pause 100

Receive	Data:84 A9 61 00 02 30 7F 00
Receive	Data:84 A9 61 00 02 30 1B 05
Receive	Data:84 A9 61 00 02 30 7C D2
Receive	Data:84 A9 61 00 04 30 76 05 05 05
Receive	Data:84 A9 61 00 04 30 50 FF FF F6
Receive	Data:84 A9 61 00 04 30 51 5F 21 C7
Receive	Data:84 A9 61 00 05 30 7D 06 AA AA AA
Receive	Data:84 A9 61 00 05 30 7E 06 23 45 67
Receive	Data:84 A9 61 00 02 30 27 02
pause 1500
Command ID:	DMR_CALL_STOP
Send	Command: 84 A9 61 00 01 03 21 00
Receive	Data:84 A9 61 00 02 03 21 00
Receive	Data:84 A9 61 00 02 30 1B 04
Receive	Data:84 A9 61 00 02 30 7B d2
Receive	Data:84 A9 61 00 01 30 4B
Receive	Data:84 A9 61 00 02 20 17 0A
Pause 360
//Receive	Data:84 A9 61 00 02 30 1B 08
//Command ID:	CARRIER_LOST
//Send	Command: 84 A9 61 00 02 03 19 01
//Receive	Data:84 A9 61 00 02 03 19 00

Command ID:	WORK_MODE_IDLE
Send	Command: 84 A9 61 00 04 00 18 00 00 00
Receive	Data:84 A9 61 00 02 00 18 00
Command ID:	CARRIER_LOST
Send	Command: 84 A9 61 00 02 03 19 00
Receive	Data:84 A9 61 00 02 03 19 00

Command ID:	WORK_MODE_TX
Send	Command: 84 A9 61 00 04 00 18 03 00 00
Receive	Data:84 A9 61 00 02 00 18 00
Command ID: DPMR_CALLED_ID
Send command: 84 A9 61 00 05 05 7d  07 aa aa aa
Receive Data: 84 A9 61 00 02 05 7d 00
Command ID:	OWNID_BCD
Send	Command: 84 A9 61 00 05 05 7e 07 23 45 67 
Receive	Data:84 A9 61 00 02 05 7e 00
Command ID:	DMR_CARRIER_READY
Send	Command: 84 A9 61 00 02 03 19 {READY_VAR}
Receive	Data:84 A9 61 00 02 03 19 00
pause 100

Command ID:	DMR_CALL_START
Send	Command: 84 A9 61 00 01 05 78
Receive	Data:84 A9 61 00 02 05 78 00
pause 400

Receive	Data:84 A9 61 00 02 30 7F 00
Receive	Data:84 A9 61 00 02 30 1B 04
Receive	Data:84 A9 61 00 02 30 7b D1
Receive	Data:84 A9 61 00 04 30 76 05 05 05
Receive	Data:84 A9 61 00 04 30 50 FF FF F7
Receive	Data:84 A9 61 00 04 30 51 6E 64 07
Receive	Data:84 A9 61 00 05 30 7d 07 AA AA AA
Receive	Data:84 A9 61 00 05 30 7e 07 23 45 67
Receive	Data:84 A9 61 00 02 30 27 02
pause 1500
Command ID:	DMR_CALL_STOP
Send	Command: 84 A9 61 00 01 03 21 00
Receive	Data:84 A9 61 00 02 03 21 00
Receive	Data:84 A9 61 00 02 30 1B 04
Receive	Data:84 A9 61 00 02 30 7B d2
Receive	Data:84 A9 61 00 01 30 4B
Receive	Data:84 A9 61 00 02 20 17 0A
Pause 360
//Receive	Data:84 A9 61 00 02 30 1B 08
//Command ID:	CARRIER_LOST
//Send	Command: 84 A9 61 00 02 03 19 01
//Receive	Data:84 A9 61 00 02 03 19 00

Command ID:	WORK_MODE_IDLE
Send	Command: 84 A9 61 00 04 00 18 00 00 00
Receive	Data:84 A9 61 00 02 00 18 00
Command ID:	CARRIER_LOST
Send	Command: 84 A9 61 00 02 03 19 00
Receive	Data:84 A9 61 00 02 03 19 00

Command ID:	WORK_MODE_TX
Send	Command: 84 A9 61 00 04 00 18 03 00 00
Receive	Data:84 A9 61 00 02 00 18 00
Command ID: DPMR_CALLED_ID
Send command: 84 A9 61 00 05 05 7d  08 aa aa aa
Receive Data: 84 A9 61 00 02 05 7d 00
Command ID:	OWNID_BCD
Send	Command: 84 A9 61 00 05 05 7e 08 23 45 67 
Receive	Data:84 A9 61 00 02 05 7e 00
Command ID:	DMR_CALL_START
Send	Command: 84 A9 61 00 01 05 78
Receive	Data:84 A9 61 00 02 05 78 00
pause 400
Command ID:	DMR_CARRIER_READY
Send	Command: 84 A9 61 00 02 03 19 {READY_VAR}
Receive	Data:84 A9 61 00 02 03 19 00
pause 100

Receive	Data:84 A9 61 00 02 30 7F 00
Receive	Data:84 A9 61 00 02 30 1B 05
Receive	Data:84 A9 61 00 02 30 7C D2
Receive	Data:84 A9 61 00 04 30 76 05 05 05
Receive	Data:84 A9 61 00 04 30 50 FF FF F8
Receive	Data:84 A9 61 00 04 30 51 7D A6 47
Receive	Data:84 A9 61 00 05 30 7D 08 AA AA AA
Receive	Data:84 A9 61 00 05 30 7E 08 23 45 67
Receive	Data:84 A9 61 00 02 30 27 02
pause 1500
Command ID:	DMR_CALL_STOP
Send	Command: 84 A9 61 00 01 03 21 00
Receive	Data:84 A9 61 00 02 03 21 00
Receive	Data:84 A9 61 00 02 30 1B 04
Receive	Data:84 A9 61 00 02 30 7B d2
Receive	Data:84 A9 61 00 01 30 4B
Receive	Data:84 A9 61 00 02 20 17 0A
Pause 360
//Receive	Data:84 A9 61 00 02 30 1B 08
//Command ID:	CARRIER_LOST
//Send	Command: 84 A9 61 00 02 03 19 01
//Receive	Data:84 A9 61 00 02 03 19 00

Command ID:	WORK_MODE_IDLE
Send	Command: 84 A9 61 00 04 00 18 00 00 00
Receive	Data:84 A9 61 00 02 00 18 00
Command ID:	CARRIER_LOST
Send	Command: 84 A9 61 00 02 03 19 00
Receive	Data:84 A9 61 00 02 03 19 00

Command ID:	WORK_MODE_TX
Send	Command: 84 A9 61 00 04 00 18 03 00 00
Receive	Data:84 A9 61 00 02 00 18 00
Command ID: DPMR_CALLED_ID
Send command: 84 A9 61 00 05 05 7d  09 aa aa aa
Receive Data: 84 A9 61 00 02 05 7d 00
Command ID:	OWNID_BCD
Send	Command: 84 A9 61 00 05 05 7e 09 23 45 67 
Receive	Data:84 A9 61 00 02 05 7e 00
Command ID:	DMR_CARRIER_READY
Send	Command: 84 A9 61 00 02 03 19 {READY_VAR}
Receive	Data:84 A9 61 00 02 03 19 00
pause 100
Command ID:	DMR_CALL_START
Send	Command: 84 A9 61 00 01 05 78
Receive	Data:84 A9 61 00 02 05 78 00
pause 400



Receive	Data:84 A9 61 00 02 30 7F 00
Receive	Data:84 A9 61 00 02 30 1B 04
Receive	Data:84 A9 61 00 02 30 7b D1
Receive	Data:84 A9 61 00 04 30 76 05 05 05
Receive	Data:84 A9 61 00 04 30 50 FF FF F9
Receive	Data:84 A9 61 00 04 30 51 8C E8 87
Receive	Data:84 A9 61 00 05 30 7d 09 AA AA AA
Receive	Data:84 A9 61 00 05 30 7e 09 23 45 67
Receive	Data:84 A9 61 00 02 30 27 02
pause 1500
Command ID:	DMR_CALL_STOP
Send	Command: 84 A9 61 00 01 03 21 00
Receive	Data:84 A9 61 00 02 03 21 00
Receive	Data:84 A9 61 00 02 30 1B 04
Receive	Data:84 A9 61 00 02 30 7B d2
Receive	Data:84 A9 61 00 01 30 4B
Receive	Data:84 A9 61 00 02 20 17 0A
Pause 360
//Receive	Data:84 A9 61 00 02 30 1B 08
//Command ID:	CARRIER_LOST
//Send	Command: 84 A9 61 00 02 03 19 01
//Receive	Data:84 A9 61 00 02 03 19 00

Command ID:	WORK_MODE_IDLE
Send	Command: 84 A9 61 00 04 00 18 00 00 00
Receive	Data:84 A9 61 00 02 00 18 00
Command ID:	CARRIER_LOST
Send	Command: 84 A9 61 00 02 03 19 00
Receive	Data:84 A9 61 00 02 03 19 00

Command ID:	WORK_MODE_TX
Send	Command: 84 A9 61 00 04 00 18 03 00 00
Receive	Data:84 A9 61 00 02 00 18 00
Command ID: DPMR_CALLED_ID
Send command: 84 A9 61 00 05 05 7d  0a aa aa aa
Receive Data: 84 A9 61 00 02 05 7d 00
Command ID:	OWNID_BCD
Send	Command: 84 A9 61 00 05 05 7e 01 23 45 67 
Receive	Data:84 A9 61 00 02 05 7e 00
Command ID:	DMR_CALL_START
Send	Command: 84 A9 61 00 01 05 78
Receive	Data:84 A9 61 00 02 05 78 00
pause 400
//Command ID:	DPMR_DATA_FRAME
//Send	Command: 84 A9 61 00 0c 05 43 01 09 00 00 00 FF FF FF 00 00 01
//Receive	Command:84 A9 61 00 01 20 43 
//Command ID:	DPMR_DATA_FRAME
//Send	Command: 84 A9 61 00 0c 05 43 11 09 00 00 00 FF FF FF 00 00 01
//Receive	Command:84 A9 61 00 01 20 43 
Command ID:	DMR_CARRIER_READY
Send	Command: 84 A9 61 00 02 03 19 {READY_VAR}
Receive	Data:84 A9 61 00 02 03 19 00
pause 100

Receive	Data:84 A9 61 00 02 30 7F 00
Receive	Data:84 A9 61 00 02 30 1B 05
Receive	Data:84 A9 61 00 02 30 7C D2
Receive	Data:84 A9 61 00 04 30 76 05 05 05
Receive	Data:84 A9 61 00 04 30 50 FF FF FF
Receive	Data:84 A9 61 00 04 30 51 12 D6 87
Receive	Data:84 A9 61 00 05 30 7D 0A AA AA AA
Receive	Data:84 A9 61 00 05 30 7e 01 23 45 67
Receive	Data:84 A9 61 00 02 30 27 02
pause 1500
Command ID:	DMR_CALL_STOP
Send	Command: 84 A9 61 00 01 03 21 00
Receive	Data:84 A9 61 00 02 03 21 00
Receive	Data:84 A9 61 00 02 30 1B 04
Receive	Data:84 A9 61 00 02 30 7B d2
Receive	Data:84 A9 61 00 01 30 4B
Receive	Data:84 A9 61 00 02 20 17 0A
Pause 360
//Receive	Data:84 A9 61 00 02 30 1B 08
//Command ID:	CARRIER_LOST
//Send	Command: 84 A9 61 00 02 03 19 01
//Receive	Data:84 A9 61 00 02 03 19 00

Command ID:	WORK_MODE_IDLE
Send	Command: 84 A9 61 00 04 00 18 00 00 00
Receive	Data:84 A9 61 00 02 00 18 00

