//Verison=2.2
//Example,Don't Delete flowing text!
//Button NIMI // Generator NIMI 
//Button NIMI 100 // Generator NIMI and Delay 100ms, 100 not is nessary
//Button INT0 // Generator INT0 and Delay 200ms
//Button RESETAMBE3000
//Button RESET3252
//Send 1 command, Receive 2 response with one is not verify.
//Command ID: CARRIER_LOST // necessary!
//Summary  // not essential, 
//Send command: 61 00 02 00 19 00 // necessary!
//Pause=300 // not essential, unit: ms; Pause 300ms after Send command
//Timeout=100 // not essential, unit: ms; if not receive '84 A9 61 ...' in 100ms after send command, Timeout error will happen!
//*Receive Data: 61 00 02 51 19 00 // not essential, receive but not verify
//Receive Data: 61 00 02 51 19 20 // not essential, receive and verify 
//.Set x = AA B0  -- Define var x ; Added in ver2.2
// ... 61 00 02 00 19 {x}   --- use the defined var, The {x} will be replaced with AA B0 
//
.Set READY_VAR = 01
//Simultaneous data call
/*Pause 2000
Command ID:	NXDN_SR
Send	Command: 84 A9 61 00 02 06 77 01
Receive Data:   84 A9 61 00 02 06 77 00 
Command ID:	NXDN_CALL_OPTION
Send	Command: 84 A9 61 00 06 06 47 82 00 00 00 00
Receive Data:   84 A9 61 00 02 06 47 00
Pause 1000
Command ID:	WORK_MODE_DUPLEX
Send	Command: 84 A9 61 00 04 00 18 03 00 00 00
Receive	Data:84 A9 61 00 02 00 18 00
Command ID:	PROCESS_MODE
Send	Command: 84 A9 61 00 02 00 1A 02
Receive	Data:84 A9 61 00 02 00 1A 00
Command ID:	CARRIER_READY
Send	Command: 84 A9 61 00 02 03 19 01
Receive	Data:84 A9 61 00 02 03 19 00
Command ID:	NXDN_DATA_FRAME
Send command: 84 a9 61 00 11 00 77 01 43 a0 00 0b 40 01 00 20 00 01 27 0f 00 00 00 00 
Receive Data: 84 a9 61 00 01 20 43
Command ID:   NXDN_DATA_FRAME
Send command: 84 a9 61 00 0e 00 43 c0 00 0a 56 01 00 20 00 01 00 01 00 00
Receive Data: 84 a9 61 00 01 20 43*/
//Receive Data: 84 A9 61 00 02 30 1B 09
//Receive Data: 84 A9 61 00 24 30 77 01 43 00 00 1E 40 10 00 00 00 00 00 00 00 00 01 00 20 00 01 27 0F 00 00 00 01 00 20 00 01 27 0F 00 00 00
//Pause 20
//Receive Data: 84 A9 61 00 24 30 77 01 43 00 00 1E 56 01 00 20 00 01 00 01 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00
//Receive Data:   84 A9 61 00 10 30 77 01 43 00 00 0A 56 01 00 20 00 01 00 01 00 00
//Pause 1000
Command ID: DIGC_DATA_FRAME
Send command: 84 a9 61 00 19 00 43 b0 00 15 50 38 00 80 00 01 00 02 40 81 04 39 11 00 00 00 00 00 00 00 00
Receive Data: 84 a9 61 00 01 20 43
//Pause 80
//Receive Data: 84 A9 61 00 24 30 77 01 43 00 00 1E 50 01 40 00 00 00 00 00 00 00 38 00 80 00 01 00 02 00 81 04 39 11 00 00 00 00 00 00 00 00
//Command ID: NXDN_DATA_FRAME
//Send command: 84 a9 61 00 11 00 77 c1 43 a0 00 0b 40 08 00 20 07 26 27 0f 00 00 00 00
//Receive       Data:84 a9 61 00 01 20 43
//Pause 120
//Receive Data: 84 A9 61 00 02 20 17 0A
//Receive Data: 84 A9 61 00 24 30 77 01 43 00 00 1E 40 10 00 00 00 00 00 00 00 00 08 00 20 07 26 27 0F 00 00 00 08 00 20 07 26 27 0F 00 00 00
//Command ID: CARRIER_LOST
//Send command: 84 A9 61 00 02 00 19 00
//Receive Data: 84 A9 61 00 02 00 19 00